# This udev rule is for any devices that should enter automatic suspend
# but are not already included in generated rules from Chromium OS via
# tools/make-autosuspend-rules.py
#

ACTION!="add", GOTO="autosuspend_manual_end"
SUBSYSTEM!="usb", GOTO="autosuspend_manual_end"

SUBSYSTEM=="usb", GOTO="autosuspend_manual_usb"

# USB rules
LABEL="autosuspend_manual_usb"
GOTO="autosuspend_manual_end"

# Enable autosuspend
LABEL="autosuspend_manual_enable"
TEST=="power/control", ATTR{power/control}="auto", GOTO="autosuspend_manual_end"

LABEL="autosuspend_manual_end"
